

TRAXXAS Pro Modified Kit Number: 104354-74

**Chassis:** only legal chassis is Traxxas #5832 Black

**Bumpers:** only Factory Traxxas bumpers permitted. Traxxas# 5836, 5836P

**Body:** the only legal body is traxxas #10411-

factory interior is required, can be painted

Numbers are required to be present on the body on both sides of the car and roof.

**Suspension:** All parts are to remain factory equipped besides approved Traxxas partslistbelow.

Aluminum turnbuckles Traxxas# 3139X, 3139P, 3139G, 3139T, 3139A

Heavy duty Suspension arms Traxxas# 3631X, 3631P, 3631G, 3631T, 3631A

Caster Blocks Traxxas# 9136, 9136-Gray, 9136-Grn, 9136-Red, 9136-Blue

Steering Blocks Traxxas# 9137-Blue, 9137-Green, 9137-Red, 9137-Gray, 9137.

Carriers Traxxas# 9150-GRN, 9150-BLU, 9150-RED, 9150

Aluminum Nut, flanged, serrated Traxxas# 1747X, 1747P, 1747G, 1747T, 1747A

**Shocks:** Factory equipped shocks only permitted.

**shock oil:** Any shock oil and weight can be used.

**Springs:** Traxxas White series only Traxxas# 5427, 5428, 5429, 5430, 5432, 5433,

**Steering:** the only servo saver allowed is Traxxas# 3744. Pinning the servo savor is permitted.

**Servo:** Traxxas# 2050, 2075X, 2075R (servo) and Traxxas 2072x (gears) are allowed as alternative parts/servo are the only permitted servos/parts.

**Steering Bellcranks:** Traxxas # 3743X, 3743P, 3743T, 3743G, 3743A are permitted.

**Electronics:** Open ESC, Open Motor.

**BATTERY:** 2S LIPO BATTERY, MAX VOLTAGE CHARGED 8.6 VOLTS. Shorty packs allowed.

**Transmitter/Receiver:** Any surface transmitter and receiver is permitted.

**Transmission:** Factory Equipped Transmission permitted. Traxxas# 9495

**Engine Plate:** Factory Equipped engine plates only Traxxas# 9490A, 9490T, 9490G, 9490X, 9490P, 9490R

**GEARS:**  Open

**Tires:** Open

**Tire Glue:** Permitted

**Tire prep:** Permitted

**ALL OTHER PARTS ARE TO REMAIN BOX STOCK IF ITS NOT COVERED IN THE RULES CONSIDER IT ILLEGAL.**